Mar 03 11:20:26.132 VTTY: Console port: waiting connection on tcp port 5002 for protocol IPv4 (FD 8)
Mar 03 11:20:26.132 CONSOLE: console managed by I/O board
Mar 03 11:20:26.600 C7200_BOOT: starting instance (CPU0 PC=0xffffffffbfc00000,idle_pc=0x62cc930c,JIT on)
Mar 03 11:20:26.600 CPU0: CPU_STATE: Starting CPU (old state=2)...
Mar 03 11:20:26.740 ROM: Microcode has started.
Mar 03 11:20:26.740 ROM: trying to read bootvar 'WARM_REBOOT'
Mar 03 11:20:26.740 CPU0: IO_FPGA: read from addr 0x3a0, pc=0xffffffff82c75d54 (size=2)
Mar 03 11:20:26.740 ROM: unhandled syscall 0x00000032 at pc=0x631755f4 (a1=0x63963394,a2=0x643a6cac,a3=0x6558e400)
Mar 03 11:20:26.740 CPU0: IO_FPGA: read from addr 0x224, pc=0x62c790b4 (size=1)
Mar 03 11:20:27.037 ROM: trying to read bootvar 'IOMEM_SIZE'
Mar 03 11:20:27.037 ROM: trying to set bootvar 'IOMEM_SIZE='
Mar 03 11:20:27.037 ROM: unhandled syscall 0x00000038 at pc=0x631755f4 (a1=0x80007db8,a2=0x643a6cac,a3=0x63f40f09)
Mar 03 11:20:27.037 ROM: trying to read bootvar 'RANDOM_NUM'
Mar 03 11:20:27.037 ROM: trying to read bootvar 'RANDOM_NUM'
Mar 03 11:20:27.068 CPU0: IO_FPGA: write to addr 0x398, value=0x2000000, pc=0x62c79e44 (size=4)
Mar 03 11:20:27.068 CPU0: IO_FPGA: write to addr 0x398, value=0x0, pc=0x62c79e48 (size=4)
Mar 03 11:20:27.068 CPU0: MP_FPGA: reading 0x78 at pc=0x62c79ec0
Mar 03 11:20:27.068 CPU0: MP_FPGA: writing reg 0x78 at pc=0x62c79ed0 (data=0xff)
Mar 03 11:20:27.068 CPU0: MP_FPGA: writing reg 0x70 at pc=0x62cbeffc (data=0x7e)
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'gt64120' at pc=0x62ca1528: bus=0,device=0,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'gt64120' at pc=0x62ca152c: bus=0,device=0,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'gt64120' at pc=0x62ca13bc: bus=0,device=0,function=0,reg=0x08
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x10
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x10
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x90
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x90
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x10000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x14
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x10000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x14
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x10000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x94
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x10000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x94
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x14000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x20
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x14000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x20
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x14000000) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0xa0
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x14000000) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0xa0
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000146) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000146) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000146) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x84
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000146) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x84
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000000f) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x0c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000000f) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x0c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000000f) for device 'gt64120' at pc=0x62ca1cd4: bus=0,device=0,function=0,reg=0x8c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000000f) for device 'gt64120' at pc=0x62ca1cd8: bus=0,device=0,function=0,reg=0x8c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xc0000000) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x10).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xc0000000) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x10).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xc0000000) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x90).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xc0000000) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x90).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xd0000000) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x14).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xd0000000) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x14).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xd0000000) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x94).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xd0000000) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x94).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000000c0) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x1c).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000000c0) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x1c).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000000c0) for unknown device at pc=0x62ca1cd4 (bus=0,device=0,function=1,reg=0x9c).
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000000c0) for unknown device at pc=0x62ca1cd8 (bus=0,device=0,function=1,reg=0x9c).
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'dec21050' at pc=0x62ca1528: bus=0,device=1,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'dec21050' at pc=0x62ca152c: bus=0,device=1,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'dec21050' at pc=0x62ca1528: bus=0,device=1,function=0,reg=0x40
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'dec21050' at pc=0x62ca152c: bus=0,device=1,function=0,reg=0x40
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000147) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000147) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00002e10) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x0c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00002e10) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x0c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x18020100) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x18
Mar 03 11:20:27.068 PCI: PCI bridge 0,1,0 -> pri: 00, sec: 01, sub: 02
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x18020100) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x18
Mar 03 11:20:27.068 PCI: PCI bridge 0,1,0 -> pri: 00, sec: 01, sub: 02
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xffff3f00) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x1c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0xffff3f00) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x1c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x48704000) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x20
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x48704000) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x20
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000ff00) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x24
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x0000ff00) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x24
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00030000) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x3c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00030000) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x3c
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00100000) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x40
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00100000) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x40
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00009020) for device 'dec21050' at pc=0x62ca1c94: bus=0,device=1,function=0,reg=0x44
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00009020) for device 'dec21050' at pc=0x62ca1ca0: bus=0,device=1,function=0,reg=0x44
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'clpd6729' at pc=0x62ca1528: bus=2,device=16,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: read request for device 'clpd6729' at pc=0x62ca152c: bus=2,device=16,function=0,reg=0x00
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000001c3) for device 'clpd6729' at pc=0x62ca1c94: bus=2,device=16,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x000001c3) for device 'clpd6729' at pc=0x62ca1ca0: bus=2,device=16,function=0,reg=0x04
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000400) for device 'clpd6729' at pc=0x62ca1c94: bus=2,device=16,function=0,reg=0x10
Mar 03 11:20:27.068 CPU0: PCI: write request (data=0x00000400) for device 'clpd6729' at pc=0x62ca1ca0: bus=2,device=16,function=0,reg=0x10
Mar 03 11:20:27.068 ROM: trying to read bootvar 'BOOTBLOT'
Mar 03 11:20:28.222 CPU0: JIT: partial JIT flush (count=834)
Mar 03 11:20:28.238 ROM: trying to read bootvar 'PRST_VBL_DEBUG'
Mar 03 11:20:28.238 ROM: trying to read bootvar 'PRST_IFS_PRFX'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'BOOT'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'CONFIG_FILE'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'BOOTLDR'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'RSHELF'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'DSHELF'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'DSHELFINFO'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'RESET_COUNTER'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'CHRG_LOCRECSN'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'CHRG_ID'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'SLOTCACHE'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'DIAG'
Mar 03 11:20:28.347 ROM: trying to read bootvar 'WARM_REBOOT'
Mar 03 11:20:28.347 ROM: unhandled syscall 0x00000087 at pc=0x631755f4 (a1=0x64615038,a2=0x651aeb98,a3=0x00000401)
Mar 03 11:20:29.408 ROM: unhandled syscall 0x0000007c at pc=0x631755f4 (a1=0x643a2298,a2=0x0000000a,a3=0x64bc9378)
Mar 03 11:20:29.408 ROM: unhandled syscall 0x0000007c at pc=0x631755f4 (a1=0x61e4be68,a2=0x6564b2f4,a3=0x6564b30c)
Mar 03 11:20:29.408 CPU0: PCI: read request for device 'gt64120' at pc=0x62cc543c: bus=0,device=0,function=0,reg=0x08
Mar 03 11:20:29.408 CPU0: CLPD6729: ext reg index 0x03 at pc=0x62cceaf4
Mar 03 11:20:29.408 CPU0: CLPD6729: ext reg index 0x03 at pc=0x62cceaf4
Mar 03 11:20:29.423 CPU0: CLPD6729: ext reg index 0x09 at pc=0x62cceaf4
Mar 03 11:20:29.423 CPU0: CLPD6729: ext reg index 0x09 at pc=0x62cceaf4
Mar 03 11:20:29.423 CPU0: CLPD6729: ext reg index 0x05 at pc=0x62cceaf4
Mar 03 11:20:29.423 CPU0: CLPD6729: ext reg index 0x05 at pc=0x62cceaf4
Mar 03 11:20:29.470 ROM: trying to read bootvar 'PROCESS_ACCOUNTING'
Mar 03 11:20:29.470 ROM: trying to read bootvar 'PRST_VBL_SHOW'
Mar 03 11:20:29.470 ROM: trying to read bootvar 'PRST_VBL_NUKE'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_DEBUG'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_CMAP_DEBUG'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_PMAP_DEBUG'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_STANDBY_DEBUG'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_MSG_INTF_DEBUG'
Mar 03 11:20:29.579 ROM: trying to read bootvar 'QOS_HA_ISSU_DEBUG'
Mar 03 11:20:29.579 Calendar: reset
Mar 03 11:20:29.595 ROM: trying to set bootvar 'BSI=0'
Mar 03 11:20:29.689 CPU0: JIT: flushing data structures (compiled pages=968)
Mar 03 11:20:29.704 ROM: trying to read bootvar 'CONFIG_FILE'
Mar 03 11:20:29.720 ROM: trying to read bootvar 'BOOTLDR'
Mar 03 11:20:29.860 CPU0: MP_FPGA: writing reg 0x70 at pc=0x62cc33f4 (data=0x2)
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca1528: bus=0,device=7,function=0,reg=0x00
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca152c: bus=0,device=7,function=0,reg=0x00
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca1528: bus=0,device=7,function=0,reg=0x08
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca152c: bus=0,device=7,function=0,reg=0x08
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca1528: bus=0,device=7,function=0,reg=0x00
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca152c: bus=0,device=7,function=0,reg=0x00
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca1528: bus=0,device=7,function=0,reg=0x40
Mar 03 11:20:30.047 CPU0: PCI: read request for device 'dec21150' at pc=0x62ca152c: bus=0,device=7,function=0,reg=0x40
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0xffff0000) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x04
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0xffff0000) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x04
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00002e10) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x0c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00002e10) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x0c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x18050504) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x18
Mar 03 11:20:30.047 PCI: PCI bridge 0,7,0 -> pri: 04, sec: 05, sub: 05
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x18050504) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x18
Mar 03 11:20:30.047 PCI: PCI bridge 0,7,0 -> pri: 04, sec: 05, sub: 05
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x02805f40) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x1c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x02805f40) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x1c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x48f04880) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x20
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x48f04880) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x20
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x0001ff01) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x24
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x0001ff01) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x24
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000000) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x30
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000000) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x30
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x03030000) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x3c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x03030000) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x3c
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x02000000) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x40
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x02000000) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x40
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000000) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x64
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000000) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x64
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x000001ff) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x68
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x000001ff) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x68
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000147) for device 'dec21150' at pc=0x62ca1c94: bus=0,device=7,function=0,reg=0x04
Mar 03 11:20:30.047 CPU0: PCI: write request (data=0x00000147) for device 'dec21150' at pc=0x62ca1ca0: bus=0,device=7,function=0,reg=0x04
Mar 03 11:20:30.141 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca1528: bus=1,device=0,function=0,reg=0x00
Mar 03 11:20:30.141 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca152c: bus=1,device=0,function=0,reg=0x00
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x00000006) for device 'C7200-IO-FE(0)' at pc=0x62ca1c94: bus=1,device=0,function=0,reg=0x04
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x00000006) for device 'C7200-IO-FE(0)' at pc=0x62ca1ca0: bus=1,device=0,function=0,reg=0x04
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x480c0000) for device 'C7200-IO-FE(0)' at pc=0x62ca1c94: bus=1,device=0,function=0,reg=0x14
Mar 03 11:20:30.141 C7200-IO-FE(0): registers are mapped at 0x480c0000
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x480c0000) for device 'C7200-IO-FE(0)' at pc=0x62ca1ca0: bus=1,device=0,function=0,reg=0x14
Mar 03 11:20:30.141 C7200-IO-FE(0): registers are mapped at 0x480c0000
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x0000ff00) for device 'C7200-IO-FE(0)' at pc=0x62ca1c94: bus=1,device=0,function=0,reg=0x0c
Mar 03 11:20:30.141 CPU0: PCI: write request (data=0x0000ff00) for device 'C7200-IO-FE(0)' at pc=0x62ca1ca0: bus=1,device=0,function=0,reg=0x0c
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'gt64120' at pc=0x62ca1528: bus=0,device=0,function=0,reg=0x08
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'gt64120' at pc=0x62ca152c: bus=0,device=0,function=0,reg=0x08
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca1528: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca152c: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x48800000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=0,function=0,reg=0x14
Mar 03 11:20:30.157 PA-8E(1): registers are mapped at 0x48800000
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x48800000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=0,function=0,reg=0x14
Mar 03 11:20:30.157 PA-8E(1): registers are mapped at 0x48800000
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=0,function=0,reg=0x04
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=0,function=0,reg=0x04
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=0,function=0,reg=0x0c
Mar 03 11:20:30.157 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=0,function=0,reg=0x0c
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.157 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=0,function=0,reg=0x00
Mar 03 11:20:30.172 PA-8E(1): fetching init block at address 0x0e1c5040
Mar 03 11:20:30.172 PA-8E(1): rx_ring = 0x0e1c50a0 (64), tx_ring = 0x0e1c54e0 (128)
Mar 03 11:20:30.172 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48820000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=1,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48820000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48820000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=1,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48820000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=1,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=1,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=1,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=1,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=1,function=0,reg=0x00
Mar 03 11:20:30.172 PA-8E(1): fetching init block at address 0x0e1d8d60
Mar 03 11:20:30.172 PA-8E(1): rx_ring = 0x0e1d8dc0 (64), tx_ring = 0x0e1d9200 (128)
Mar 03 11:20:30.172 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48840000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=2,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48840000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48840000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=2,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48840000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=2,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=2,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=2,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=2,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=2,function=0,reg=0x00
Mar 03 11:20:30.172 PA-8E(1): fetching init block at address 0x0e1eca80
Mar 03 11:20:30.172 PA-8E(1): rx_ring = 0x0e1ecae0 (64), tx_ring = 0x0e1ecf20 (128)
Mar 03 11:20:30.172 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48860000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=3,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48860000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x48860000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=3,function=0,reg=0x14
Mar 03 11:20:30.172 PA-8E(1): registers are mapped at 0x48860000
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=3,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=3,function=0,reg=0x04
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=3,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=3,function=0,reg=0x0c
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.172 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=3,function=0,reg=0x00
Mar 03 11:20:30.188 PA-8E(1): fetching init block at address 0x0e2007a0
Mar 03 11:20:30.188 PA-8E(1): rx_ring = 0x0e200800 (64), tx_ring = 0x0e200c40 (128)
Mar 03 11:20:30.188 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x48880000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=4,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x48880000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x48880000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=4,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x48880000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=4,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=4,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=4,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=4,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=4,function=0,reg=0x00
Mar 03 11:20:30.188 PA-8E(1): fetching init block at address 0x0e2144c0
Mar 03 11:20:30.188 PA-8E(1): rx_ring = 0x0e214520 (64), tx_ring = 0x0e214960 (128)
Mar 03 11:20:30.188 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x488a0000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=5,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x488a0000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x488a0000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=5,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x488a0000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=5,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=5,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=5,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=5,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=5,function=0,reg=0x00
Mar 03 11:20:30.188 PA-8E(1): fetching init block at address 0x0e2281e0
Mar 03 11:20:30.188 PA-8E(1): rx_ring = 0x0e228240 (64), tx_ring = 0x0e228680 (128)
Mar 03 11:20:30.188 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x488c0000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=6,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x488c0000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x488c0000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=6,function=0,reg=0x14
Mar 03 11:20:30.188 PA-8E(1): registers are mapped at 0x488c0000
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=6,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=6,function=0,reg=0x04
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=6,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=6,function=0,reg=0x0c
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.188 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=6,function=0,reg=0x00
Mar 03 11:20:30.203 PA-8E(1): fetching init block at address 0x0e23bf00
Mar 03 11:20:30.203 PA-8E(1): rx_ring = 0x0e23bf60 (64), tx_ring = 0x0e23c3a0 (128)
Mar 03 11:20:30.203 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x488e0000) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=7,function=0,reg=0x14
Mar 03 11:20:30.203 PA-8E(1): registers are mapped at 0x488e0000
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x488e0000) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=7,function=0,reg=0x14
Mar 03 11:20:30.203 PA-8E(1): registers are mapped at 0x488e0000
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=7,function=0,reg=0x04
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x00000006) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=7,function=0,reg=0x04
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1c94: bus=5,device=7,function=0,reg=0x0c
Mar 03 11:20:30.203 CPU0: PCI: write request (data=0x0000ff00) for device 'PA-8E(1)' at pc=0x62ca1ca0: bus=5,device=7,function=0,reg=0x0c
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca1528: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 CPU0: PCI: read request for device 'PA-8E(1)' at pc=0x62ca152c: bus=5,device=7,function=0,reg=0x00
Mar 03 11:20:30.203 PA-8E(1): fetching init block at address 0x0e24fc20
Mar 03 11:20:30.203 PA-8E(1): rx_ring = 0x0e24fc80 (64), tx_ring = 0x0e2500c0 (128)
Mar 03 11:20:30.203 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca1528: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.219 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca152c: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e1c5040
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e1c50a0 (64), tx_ring = 0x0e1c54e0 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e1d8d60
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e1d8dc0 (64), tx_ring = 0x0e1d9200 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e1eca80
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e1ecae0 (64), tx_ring = 0x0e1ecf20 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e2007a0
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e200800 (64), tx_ring = 0x0e200c40 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e2144c0
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e214520 (64), tx_ring = 0x0e214960 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e2281e0
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e228240 (64), tx_ring = 0x0e228680 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e23bf00
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e23bf60 (64), tx_ring = 0x0e23c3a0 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.219 PA-8E(1): fetching init block at address 0x0e24fc20
Mar 03 11:20:30.219 PA-8E(1): rx_ring = 0x0e24fc80 (64), tx_ring = 0x0e2500c0 (128)
Mar 03 11:20:30.219 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.359 CPU0: JIT: partial JIT flush (count=805)
Mar 03 11:20:30.562 CPU0: JIT: flushing data structures (compiled pages=1003)
Mar 03 11:20:30.618 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca1528: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.618 CPU0: PCI: read request for device 'C7200-IO-FE(0)' at pc=0x62ca152c: bus=1,device=0,function=0,reg=0x08
Mar 03 11:20:30.624 PA-8E(1): fetching init block at address 0x0e1c5040
Mar 03 11:20:30.624 PA-8E(1): rx_ring = 0x0e1c50a0 (64), tx_ring = 0x0e1c54e0 (128)
Mar 03 11:20:30.624 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.625 PA-8E(1): fetching init block at address 0x0e1d8d60
Mar 03 11:20:30.625 PA-8E(1): rx_ring = 0x0e1d8dc0 (64), tx_ring = 0x0e1d9200 (128)
Mar 03 11:20:30.625 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.626 PA-8E(1): fetching init block at address 0x0e1eca80
Mar 03 11:20:30.626 PA-8E(1): rx_ring = 0x0e1ecae0 (64), tx_ring = 0x0e1ecf20 (128)
Mar 03 11:20:30.626 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.627 PA-8E(1): fetching init block at address 0x0e2007a0
Mar 03 11:20:30.627 PA-8E(1): rx_ring = 0x0e200800 (64), tx_ring = 0x0e200c40 (128)
Mar 03 11:20:30.627 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.627 PA-8E(1): fetching init block at address 0x0e2144c0
Mar 03 11:20:30.627 PA-8E(1): rx_ring = 0x0e214520 (64), tx_ring = 0x0e214960 (128)
Mar 03 11:20:30.627 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.628 PA-8E(1): fetching init block at address 0x0e2281e0
Mar 03 11:20:30.628 PA-8E(1): rx_ring = 0x0e228240 (64), tx_ring = 0x0e228680 (128)
Mar 03 11:20:30.628 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.629 PA-8E(1): fetching init block at address 0x0e23bf00
Mar 03 11:20:30.629 PA-8E(1): rx_ring = 0x0e23bf60 (64), tx_ring = 0x0e23c3a0 (128)
Mar 03 11:20:30.629 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:30.630 PA-8E(1): fetching init block at address 0x0e24fc20
Mar 03 11:20:30.630 PA-8E(1): rx_ring = 0x0e24fc80 (64), tx_ring = 0x0e2500c0 (128)
Mar 03 11:20:30.630 PA-8E(1): CSR0 = 0x0101
Mar 03 11:20:32.705 CPU0: JIT: partial JIT flush (count=744)
Mar 03 11:20:32.892 CPU0: JIT: flushing data structures (compiled pages=1020)
Mar 03 11:20:32.923 ROM: trying to read bootvar 'TPM_DEBUG'
Mar 03 11:20:33.095 CPU0: JIT: partial JIT flush (count=855)
Mar 03 11:20:33.344 CPU0: JIT: flushing data structures (compiled pages=1049)
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_EVENT_ALL'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_EVENT_FROM'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_EVENT_TO'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_EVENT'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_CLIENT_ALL'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_CLIENT_FROM'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_CLIENT_TO'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_CLIENT'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_LEVEL'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_DATABASE_RUNTIME'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_DATABASE_TEMPLATE'
Mar 03 11:20:33.407 ROM: trying to read bootvar 'CPL_EVENT_DBG_FILTERING'
Mar 03 11:20:35.669 CPU0: JIT: partial JIT flush (count=779)
Mar 03 11:20:36.059 CPU0: JIT: flushing data structures (compiled pages=1045)
Mar 03 11:20:36.418 ROM: unhandled syscall 0x0000001a at pc=0x631755f4 (a1=0x00000000,a2=0x00000000,a3=0x6532907c)
Mar 03 11:20:36.418 ROM: unhandled syscall 0x00000009 at pc=0x631755f4 (a1=0x639634a0,a2=0x643a6cac,a3=0x6532907c)
Mar 03 11:20:36.418 ROM: unhandled syscall 0x00000082 at pc=0x631755f4 (a1=0x63963384,a2=0x643a6cac,a3=0x00000003)
Mar 03 11:20:36.418 ROM: unhandled syscall 0x00000039 at pc=0x631755f4 (a1=0x63963478,a2=0x643a6cac,a3=0x00000003)
Mar 03 11:20:36.418 ROM: trying to read bootvar 'RET_2_RTS'
Mar 03 11:20:36.418 ROM: trying to read bootvar 'IOMEM_SIZE'
Mar 03 11:20:36.418 ROM: trying to read bootvar 'WARM_REBOOT'
Mar 03 11:20:36.418 ROM: trying to read bootvar 'RELOAD_TYPE'
Mar 03 11:20:36.418 ROM: unhandled syscall 0x00000047 at pc=0x631755f4 (a1=0x63a1b024,a2=0x650bde58,a3=0x00000101)
Mar 03 11:20:36.496 CPU0: JIT: partial JIT flush (count=794)
Mar 03 11:20:36.648 ROM: trying to set bootvar 'BSI=0'
Mar 03 11:20:36.648 ROM: trying to set bootvar 'BSI=-1'
Mar 03 11:20:36.753 CPU0: JIT: flushing data structures (compiled pages=1099)
Mar 03 11:20:37.190 CPU0: JIT: partial JIT flush (count=743)
Mar 03 11:20:37.487 ROM: trying to set bootvar 'BSI=0'
Mar 03 11:20:37.487 ROM: trying to read bootvar 'RET_2_RCALTS'
Mar 03 11:20:37.487 ROM: trying to set bootvar 'RET_2_RCALTS='
Mar 03 11:20:37.923 CPU0: JIT: flushing data structures (compiled pages=1090)
Mar 03 11:20:38.033 ROM: trying to read bootvar 'RANDOM_NUM'
Mar 03 11:20:42.616 CPU0: JIT: partial JIT flush (count=665)
Mar 03 11:22:41.071 ROM: trying to set bootvar 'RANDOM_NUM=41108690'
Mar 03 11:44:22.391 VTTY: Console port is now connected (accept_fd=8,conn_fd=15)
Mar 03 11:44:57.759 CPU0: JIT: flushing data structures (compiled pages=1503)
Mar 03 11:45:37.859 CPU0: JIT: partial JIT flush (count=770)
Mar 03 11:45:42.464 CPU0: JIT: flushing data structures (compiled pages=1545)
Mar 03 11:46:07.664 CPU0: JIT: partial JIT flush (count=780)
Mar 03 11:46:26.540 CPU0: JIT: flushing data structures (compiled pages=1560)
Mar 03 11:46:40.285 ROM: trying to read bootvar 'WARM_REBOOT'
Mar 03 11:46:40.285 ROM: trying to set bootvar 'WARM_REBOOT=FALSE'
Mar 03 11:46:40.360 CPU0: JIT: partial JIT flush (count=749)
Mar 03 11:46:40.450 CPU0: MP_FPGA: read from addr 0x0, pc=0x62c9624c
Mar 03 11:46:40.555 CPU0: JIT: flushing data structures (compiled pages=1609)
Mar 03 11:46:41.015 CPU0: JIT: partial JIT flush (count=717)
Mar 03 11:46:41.260 CPU0: JIT: flushing data structures (compiled pages=1778)
Mar 03 11:53:45.423 VTTY: Console port is now connected (accept_fd=8,conn_fd=15)
Mar 03 11:54:30.858 C7200_STOP: stopping simulation.
Mar 03 11:54:30.858 CPU0: CPU_STATE: Halting CPU (old state=0)...
Mar 03 11:54:30.883 VM: shutdown procedure engaged.
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "io_fpga"
Mar 03 11:54:30.883 DEVICE: Removal of device io_fpga, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "mp_fpga"
Mar 03 11:54:30.883 DEVICE: Removal of device mp_fpga, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "clpd6729"
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "mem_bswap"
Mar 03 11:54:30.883 DEVICE: Removal of device mem_bswap, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "rom"
Mar 03 11:54:30.883 DEVICE: Removal of device rom, fd=-1, host_addr=0x0, flags=2
Mar 03 11:54:30.883 VM_OBJECT: Shutdown of object "ram"
Mar 03 11:54:30.883 DEVICE: Removal of device ram, fd=12, host_addr=0xda3d0000, flags=2
Mar 03 11:54:30.883 MMAP: unmapping of device 'ram', fd=12, host_addr=0xda3d0000, len=0x10000000
Mar 03 11:54:30.928 VM_OBJECT: Shutdown of object "gt64120"
Mar 03 11:54:30.928 DEVICE: Removal of device gt64120, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.928 VM_OBJECT: Shutdown of object "iomem"
Mar 03 11:54:30.928 DEVICE: Removal of device iomem, fd=11, host_addr=0xea3d0000, flags=2
Mar 03 11:54:30.928 MMAP: unmapping of device 'iomem', fd=11, host_addr=0xea3d0000, len=0x10000000
Mar 03 11:54:30.938 VM_OBJECT: Shutdown of object "zero"
Mar 03 11:54:30.938 DEVICE: Removal of device zero, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.938 VM_OBJECT: Shutdown of object "nvram"
Mar 03 11:54:30.938 DEVICE: Removal of device nvram, fd=10, host_addr=0xfa3d0000, flags=9
Mar 03 11:54:30.938 MMAP: unmapping of device 'nvram', fd=10, host_addr=0xfa3d0000, len=0x80000
Mar 03 11:54:30.968 VM_OBJECT: Shutdown of object "bootflash"
Mar 03 11:54:30.968 DEVICE: Removal of device bootflash, fd=9, host_addr=0xfa450000, flags=1
Mar 03 11:54:30.968 MMAP: unmapping of device 'bootflash', fd=9, host_addr=0xfa450000, len=0x800000
Mar 03 11:54:30.968 VM_OBJECT: Shutdown of object "remote_ctrl"
Mar 03 11:54:30.968 DEVICE: Removal of device remote_ctrl, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.968 VM: removing PCI busses.
Mar 03 11:54:30.968 DEVICE: Removal of device pci_io, fd=-1, host_addr=0x0, flags=0
Mar 03 11:54:30.968 VM: deleting VTTY.
Mar 03 11:54:30.968 VTTY: Console port: closing FD 8
Mar 03 11:54:30.968 VM: deleting system CPUs.
Mar 03 11:54:30.968 CPU0: CPU_STATE: Halting CPU (old state=1)...
Mar 03 11:54:30.988 VM: shutdown procedure completed.
